MANEUVERS - Seminole
SHORT FIELD T.O.

· 0 Flap

· Hold Brakes/MAX PWR

· Rotate – 70K -1K (55K)
· Sim – Gear Up

· Climb – 82K  (56K)
· 200’ -88K  (74K)
DEPARTURE
· TALK, TALK, TALK
· Cruise CH
· CH Winds
Vmc DEMO

· CLAW AT

· 4000’ Min

· Before Landing CH

· GEAR UP

· 100K

· LEFT engine IDLE

· RIGHT Engine Max Power/Prop

· Increase Pitch 1 Deg/Sec

· Recover at Vmc/Stall/Rudder
· Reduce Power & AOA

· Return to FULL POWER

· Min Alt Loss

· 88K

DRAG DEMO

· CLAW AT

· 3000’ Min

· Before Landing CH

· GEAR UP

· 88K

· Level Flt

· Gear, Flaps 10, 25, 40

· Note power increases

· LEFT Engine IDLE 

· RIGHT Engine Max Power/Prop

· Flaps, Gear, Flaps, Flaps

· Simulate Feather (2180RPM)

· 82K then 100K

SLOW FLIGHT

· CLAW AT

· 3000’ Min 

· Before Landing CH

· Gear/Full Flaps

· 1.2 Vs1 - 68K

· HOLD ALT & Maneuver

LANDING STALL

· CLAW AT

· 3000’ Min

· Before Landing CH

· Gear/Full Flaps

· 88K descent
· Power to Idle 

· Hold descent to Horn

· Max Power; Min Alt loss

· Flaps, Gear. Flaps, Flaps

· 88K Recovery

DEPARTURE STALL

· CLAW AT

· 3000’ Min

· Before Landing CH

· GEAR UP

· 80K - Power 18” MP

· Increase Pitch to Horn

· Max Power; Min Alt loss

· Flaps, Gear. Flaps, Flaps

· 88K Recovery

ELEVATOR TRIM STALL
· CLAW AT

· 3000’ Min

· Before Landing CH

· GEAR DN
· FLAPS 25
· 88K
· Power IDLE
· Trim 
· ADD POWER
· Allow to Pitch up & Recover
STEEP TURNS

· CLAW AT

· 3000’ Min

· Before Landing CH

· GEAR UP

· 120K – 2400RPM/18” MP

EMERGENCY DESC

· Idle/Full Prop/Mixture
· Fuel Pumps ON
· Gear Down, Bank 45
· 140 Max
RECTANGULAR COURSE

TURNS ABOUT POINT

S TURNS

· CLAW AT
· 800’
· 100K

· Enter Downwind

· Hold ALT/AS

EIGHTS ON PYLONS
· CLAW AT
· 800’
· 100K

· Downwind

· 120K – 1274’

· 100K – 885’

· 90K – 717’

· SLOW = LOW

· FAST = HIGH
CHANDELLE

· CLAW AT
· 3000’ MIN
· 105K (130) Level
· Set up X Wind

· Turn into wind

· FULL POWER

· Pitch 15, Bank 30

· END 58K

LAZY EIGHT

· CLAW AT
· 3000’ MIN
· 105K (130) Level

· Trim & SET Power

· Set up X Wind

· Turn into wind

· 45 point - Pitch 15, Bank 15

· 90 point – Pitch 0, Bank 30

· 135 point – Pitch -15 Bank 15

· 180 point 105K, Original Alt
CROSS CONTROL STALL

· CLAW AT
· 3000’ MIN
· Before Landing CH
· GEAR DN
· FLAPS UP
· 72K
· Power IDLE
· Bank, Bottom Rudder
SPINS

· CLAW AT
· 6000’ MIN
· NOTE TURN REF PT
· 72K Level

· Power IDLE

· LEVEL FLT
· SPIN 2 Turns
· Recover
